**DELIVERY CHALLAN**

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| DC no:22-23QSodiem301 | | | | |  | |  | |  | date: 11/11/2022 | |  | |
| client: **Sodiem Village Panchayat** | | | | | | |  | |  | Ref: b22-23MQ311  Dated: 11-11-2022  Delivery of Material | | | |
|  | | | |
| Billing Address: Sodiem Village Panchayat Siolim Goa | | | | | | | | | |  | |  | |
|  |  |  | | | | | | |  | GSTIN: **30BBPPP8605M1Z7** | | | |
| Shipping Address: Sodiem Village Panchayat Siolim Goa | | | | | | | | | |  | |  | |
|  |  |  | | | | | | | |  |  |  | |
|  |  |  | | |  | |  | |  |  |  |  | |
|  |  |  | | |  | |  | |  |  |  |  | |
| |  |  |  | | --- | --- | --- | | **Sr. No** | **Item Description** | **Qty** | | 1 | 2 MP Day & Night Fixed Outdoor Bullet Network Camera | 35 | | 2 | Point to point access point: 802.11a/n/ac 5G Outdoor Wireless Bridge Internal 15dBi Antenna (works with CWM-F200, DWC-F256 & DWC-F2000) | 14 | | 3 | 4 MP Day & Night Varifocal Outdoor Bullet Network Camera | 2 | | 4 | 64CH 8 SATA RAID Network Video Recorder (NVR) | 1 | | 5 | 8 port manged Switch with 4 x 10/100/1000 Base-T PoE+ Ports, 1 x 10/100/1000 Base-T Port & 2 x 100/1000 Base-X SFP port. -40°C~70°C (-40°F~158°F) Operating Temperature. | 1 | | 6 | 24-Ports 10/100/1000Mbps + 4-Ports Combo GE/SFP Smart Managed Switch | 1 | | 7 | Wall Mount Rack 6U x 550 W x 450 D, with Standard accessories | 1 | | 8 | Patch Panel UTP Keystone- 24 Port- Unloaded (Cat 5e,Cat 6 & Cat 6 A ) | 9 | | 9 | Jack Cat 6 Keystone UTP - White | 116 | | 10 | Cabling with CAT 6 cable with laying | 340 | | 11 | UTP Modular Plugs Pack of 100 | 1 | | 12 | CAT6 UTP 24AWG PATCH CORD:1M,Plug 30U' Snagless | 50 | |  |  | | |  | |  | |  |  |  |  | |
|  | | |  |  | |  | |  | | | | |
|  | | |  |  | |  | |  | | | | |
|  |  |  | | |  | |  | |  |  |  |  | |
| Terms and conditions apply as per norms JPT001 | | | | | | |  | |  |  |  |  | |