**QUOTATION**

Quotation no: Datta Kare Associates 111

Date 06/05/2022

**To**

**Datta Kare Associates,**

**Goa**

Dear Sir,

Kindly check the quotation as per your requirement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SR NO** | **ITEM DESCRIPTION** | **QTY** | **PRICE** | **AMOUNT** |
| 1 | Supplying, Installing, Testing & Commissioning of Indoor PoE IP Dome Camera, minimum 5.0 mega pixel, 25m IR distance, 10/100 base T LAN, ONVIF, PoE (IEEE 802.3 af compliant), Day/ Night, Night Vision, Motion based recording, 1/3" CMOS sensor, 0.08 min. lux for colour & 0.1 lux for monochrome, 16:9 aspect ration, 2592x1520, 20 FPS, H.264 Video compression, autofocus with 2.8mm fixed lens, Contrast/ Sharpness/ White Balance/ DWDR/ Privacy masking, power supply, Wall/ False ceiling mounting with all necessary accessories. | 1 | 9600 | 9600 |
| 2 | Supplying, Installing, Testing & Commissioning of Outdoor PoE IP Bullet Camera, minimum 5.0 mega pixel, 30m IR distance, IP66, 10/100 base T LAN, ONVIF, PoE (IEEE 802.3 af compliant), Day/ Night, Night Vision, Motion based recording, 1/3" CMOS sensor, 0.08 min. lux for colour & 0.1 lux for monochrome, 16:9 aspect ration, 2592x1520, 20 FPS, H.264 Video compression, autofocus with 2.8mm fixed lens, Contrast/ Sharpness/ White Balance/ DWDR/ Privacy masking, power supply, Wall/ False ceiling mounting with all necessary accessories. | 1 | 9900 | 9900 |
| 3 | Supplying, Installing, testing & Commissioning of rack mount, ONVIF support Network Video Recorder suitable for minimum 5MP, 8 input channels for 25 FPS at minimum 4 CIF simultaneous recording in RAID 1 & H.264/MPEG/MJPEG, with continuous/ scheduled/ event and motion trigger record, minimum 4 channel min 4 CIF live playback, with Recording NVR has separate VMS software the same should be included in package and loaded on client viewing with licence for cameras. | 1 | 19800 | 19800 |
| 4 | Supplying, Installing, testing & Commissioning of rack mount, ONVIF support Network Video Recorder suitable for minimum 5MP, 16 input channels for 25 FPS at minimum 4 CIF simultaneous recording in RAID 1 & H.264/MPEG/MJPEG, with continuous/ scheduled/ event and motion trigger record, minimum 4 channel min 4 CIF live playback, with Recording NVR has separate VMS software the same should be included in package and loaded on client viewing with licence for cameras. | 1 | 28900 | 28900 |
| 5 | Supplying, Installing, testing & Commissioning of rack mount, ONVIF support Network Video Recorder suitable for minimum 5MP, 32 input channels for 25 FPS at minimum 4 CIF simultaneous recording in RAID 1 & H.264/MPEG/MJPEG, with continuous/ scheduled/ event and motion trigger record, minimum 4 channel min 4 CIF live playback, with Recording NVR has separate VMS software the same should be included in package and loaded on client viewing with licence for cameras. | 1 | 48900 | 48900 |
| 6 | Supplying, Installing, Testing & Commissioning of Wall bracket mounted professional grade 40" back lit LED screen for workstation operated panel 1920x1080 min, 16:9 aspect, 350 nits, 5000:1 contrast, 1780 H/V, VGA/DVI-D/ HDMI input, RS232C In/Out, Narrow Bezel, stereo input/ output | 1 | 48900 | 48900 |
| 7 | Supply, Installation, testing & commissioning of 6TB Surveillance Grade Hard Drive SATA 6Gb/s 128MB Cache Internal Drive, 3.5 Inch in NVR | 1 | 18000 | 18000 |

**Client scope:**

Scaffolding wherever required to be provided.

Electrification wherever necessary to be provided.

Fabrication like poles etc. to be provided.

Fabricated poles if required to be provided.

Civil work if required.

**Payment Terms**

100 % Advance

**Terms & conditions apply**.

Quotation valid for 10 days only.

Any extra item if required to be charged as actual.

Warranty as per manufacturer not valid in case of surges, fluctuation, lightening etc.to be claimed directly with the

manufacturer without involving JP TECHATRONICS.

Solution done as per recommendation and request by client hence, JP TECHATRONICS or its employees should not be held responsible for any kind of malfunctioning of the system for any reasons.

Services like data backup, searching footage, port forwarding etc. to be charged as actuals.

Service calls post installation to be charged as actuals.