|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  |  |  | **PURCHASE ORDER** | | |  |  |  |
|  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |
| Po no: 22-23 QDlink 312 | | |  |  |  | Date: 08/11/2022 | |  |
| Supplier: Dlink | | | |  |  | Quotation No :As per e-mail | | |
| Billing Address: A1, Haritaras Siddharud Sadan, Altinho Rd | | | | | |  | |  |
|  |  | St-inez Panaji - Goa 403001 | | |  | gstin: **30BBPPP8605M1Z7** | | |
| Shipping Address: 114, Gera Imperium Green, Next to | | | | | |  | |  |
|  |  | Jairam complex, Mala Panaji Goa 403001 | | | |  |  |  |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Sr. No** | **Item Description** | **Qty** | **Price** | **Amount** |
| 1 | 2 MP Day & Night Fixed Outdoor Bullet Network Camera | 35 | 2200 | 77000 |
| 2 | 802.11a/n/ac 5G Outdoor Wireless Bridge Internal 15dBi Antenna (works with CWM-F200, DWC-F256 & DWC-F2000) | 24 | 7500 | 180000 |
| 3 | 64CH 8 SATA RAID Network Video Recorder (NVR) | 1 | 45500 | 45500 |
| 4 | 8 port manged Switch with 8 x 10/100/1000 Base-T PoE+ Ports, 2 x 100/1000 Base-X SFP port.  -40°C~70°C (-40°F~158°F) Operating Temperature. | 12 | 32000 | 384000 |
| 5 | 24-Ports 10/100/1000Mbps + 4-Ports Combo GE/SFP Smart Managed Switch | 1 | 9000 | 9000 |
| 6 | Wall Mount Rack 6U x 550 W x 450 D, with Standard accessories | 1 | 3700 | 3700 |
| 7 | Patch Panel  UTP Keystone- 24 Port- Unloaded (Cat 5e,Cat 6 & Cat 6 A ) | 13 | 900 | 11700 |
| 8 | Jack Cat 6 Keystone UTP - White | 116 | 115 | 13340 |
| 9 | CAT6 UTP 23AWG Solid:305M Outdoor | 2 | 7800 | 15600 |
| 10 | UTP Modular Plugs Pack of 100 | 1 | 400 | 400 |
| 11 | CAT6 UTP 24AWG PATCH CORD:1M,Plug 30U' Snagless | 50 | 95 | 4750 |
| **Total** | | | | **744990** |
| **CGST 9%** | | | | **67049.1** |
| **SGST 9%** | | | | **67049.1** |
| **Grand Total** | | | | **879088.2** |

Terms and conditions apply as per norms JPT001

Kindly dispatch the material as per quotation mentioned

Delivery of material accepted latest by 14th November 2022.