**QUOTATION**

Quotation no: Dourado 211

Date 09/08/2022

**To**

**Mr.Dourado,**

**Nuvem Goa**

Dear Sir,

Kindly check the quotation as per your requirement.

**Hogar ZWave Solution**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Automation for Room 1 (Ground Floor)** | | | | |
| **Sr. No** | **DESCRIPTION** | **Qty** | **Price** | **Amount** |
| 1 | Cerebro-Mini(HC Mini) Gateway | 1 | 27900 | 27900 |
| 2 | 8 Touch Panel With Gold Bezel & Black Glass (IN) | 1 | 39900 | 39900 |
| 3\* | 1 channel light dimmer | 1 | 19600 | 19600 |
| 4 | Fan dimmer 1-channel fan speed control insert module with load current max 8A, compatible with standard ceiling and wall-mounted fans | 1 | 19600 | 19600 |
| 5 | 3-Node (Z-Wave) Either operates as three switch on/off / Roller shades based on selection | 3 | 19200 | 57600 |
| 6 | IR Controller(Z-Wave) | 1 | 19600 | 19600 |
| 7 | Celing mount PIR senosr (Standalone) | 1 | 4500 | 4500 |
| 8 | INSTALLATION TESTING COMMISSIONING | 1 | 15000 | 15000 |
| **Total** | | | | **203700** |
|  |  |  |  |  |
|  |  |  |  |  |
| **Automation for Room 2 (First Floor)** | | | | |
| **Sr. No** | **DESCRIPTION** | **Qty.** | **Price** | **Amount** |
| 1 | Cerebro-Mini(HC Mini) Gateway | 1 | 27900 | 27900 |
| 2 | 8 Touch Panel With Gold Bezel & Black Glass (IN) | 1 | 39900 | 39900 |
| 3\* | 1 channel light dimmer | 1 | 19600 | 19600 |
| 4 | Fan dimmer 1-channel fan speed control insert module with load current max 8A, compatible with standard ceiling and wall-mounted fans | 1 | 19600 | 19600 |
| 5 | 3-Node (Z-Wave) Either operates as three switch on/off / Roller shades based on selection | 1 | 19200 | 19200 |
| 6 | IR Controller(Z-Wave) | 1 | 19600 | 19600 |
| 7 | Celing mount PIR senosr (Standalone) | 2 | 4500 | 9000 |
| 8 | INSTALLATION TESTING COMMISSIONING | 1 | 14000 | 14000 |
| **Total** | | | | **168800** |
|  |  |  |  |  |
| **Dimming for additional light if required to be charged extra @19600/- + GST** | |  |  |  |
|  |  |  |  |  |
| **\*RJ 45 interface to be provided by client** | |  |  |  |

**Client scope:**

Scaffolding wherever required to be provided.

Electrification wherever necessary to be provided with stabilized output.

Fabrication like poles etc. to be provided.

Fabricated poles if required to be provided.

Civil work if required.

INTERNET wifi / network backbone

Gang boxes as advised and Ethernet /cat 6 cable to network db

**Payment Terms**

100 % Advance

**Company’s Bank Details**

**Bank Name:** Central Bank of India

**Account Number:** 3167002097

**Branch & IFS Code:** Panaji & CBIN0280713

**Terms & conditions apply.**

Above quoted BOQ is by considering approximate requirement, which may increase/decrease after confirmation of the actual requirement from the client.

Delivery 7 to 8 weeks from the date of receipt of technically and commercially clear purchase order.

**GST @ 18% Extra**

Validity of offer is 30 days from the date of quotation.

In case the order is finalized on us, the same will be routed through our authorized System Integrator.

Above prices & installation/configuration/programming charges are based on this configuration only.

Quotation valid for 10 days only.

Any extra item if required to be charged as actual.

Warranty as per manufacturer not valid in case of surges, fluctuation, lightening etc.to be claimed directly with the manufacturer without involving JP TECHATRONICS.

Solution done as per recommendation and request by client hence, JP TECHATRONICS or its employees should not be held responsible for any kind of malfunctioning of the system for any reasons.

Services like data backup, searching footage, port forwarding etc. to be charged as actuals.

Service calls post installation to be charged as actuals.