**QUOTATION**

Quotation no: Goa College of Engineering 106

Date 28/04/2022

**To**

**The Assistant Manager**

**Goa College of Engineering**

**Ponda Goa**

Dear Sir,

Kindly check the quotation as per your requirement.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **SR NO** | **ITEM DESCRIPTION** | **QTY** | **PRICE** | **AMOUNT** |
| 1 | CP Plus / Dahua 08-channel IP video access, Smart H.265+/Smart H.264+/H.265/H.264/MJPEG; H.265 auto switch, Max 320Mbps incoming bandwidth, 5 series professional | 1 | 24900 | 24900 |
| 2 | CP Plus / Dahua Access ANPR Camera, Adopts high-performance CMOS image sensor and processor for in-depth extraction and analysis of vehicle information 24/7 , Embraces deep learning algorithm for accurate recognition of vehicles without license plate, and vehicle model, vehicle logo, vehicle series, vehicle color, and more, Various signal, data and communication interfaces; supports connecting to extra devices, such as barrier | 1 | 54900 | 54900 |
| 3 | CP Plus / Dahua 4MP WDR IR Bullet Network Camera · H.265 codec, high compression ration, ultra-low bit rate, Built-in IR LED, max IR distance: 30 m, ROI, SMART H.264/H.265, flexible coding, applicable to various bandwidth and storage environments· Rotation mode, WDR, 3D DNR, HLC, BLC, digital watermarking | 2 | 7800 | 15600 |
| 4 | Dlink Or Similar Network Rack 2U | 1 | 2500 | 2500 |
| 5 | RJ 45 Connector with Crimping etc complete | 8 | 150 | 1200 |
| 6 | WD Purple Surveillance Hard Disk 1 TB | 1 | 4200 | 4200 |
| 7 | D link or Similar 4+2 Port POE Switch | 1 | 4460 | 4460 |
| 8 | INSTALLATION TESTING COMMISSIONING | 1 | 15000 | 15000 |
| **TOTAL** | | | | **122760** |
|  |  |  |  |  |
| **Supply and laying of cat 6 cables through PVC pipe / casing caping to be charged as actuals @ 95/- per mtr + GST** | | | | |
|  |  |  |  |  |
| **In lieu of 3\*** |  |  |  |  |
| **4MP IR Vari-focal Bullet Network Camera H.265 codec, high compression rate, ultra-low bit rate, 2.7 mm–13.5 mm, Built-in IR LED, max IR distance: 60 m, ROI, SMART H.264+/H.265+, flexible coding, applicable to various bandwidth and storage environments, Rotation mode, WDR, 3D NR, HLC, BLC, digital watermarking, applicable to various monitoring scenes, Intelligent detection: Intrusion, tripwire** | |  |  |  |
|  |  |  |  |  |
| **If required: -** |  |  |  |  |
| **1)Display 19'' @7900 + GST** | |  |  |  |
| **2) Spike Board @ 600/- + GST** | |  |  |  |
| **3) HDMI cable (3mtrs) @ 500/- + GST** | |  |  |  |
| **4) Enclosure with mounting @ 100/- + GST** | |  |  |  |

**Client scope:**

Scaffolding wherever required to be provided.

Electrification wherever necessary to be provided.

Fabrication like poles etc. to be provided.

Fabricated poles if required to be provided.

Civil work if required.

**Payment Terms**

100 % Advance

**Terms & conditions apply**.

Quotation valid for 10 days only.

GST @ 18 % Extra

Any extra item if required to be charged as actual.

Warranty as per manufacturer not valid in case of surges, fluctuation, lightening etc.to be claimed directly with the

manufacturer without involving JP TECHATRONICS.

Solution done as per recommendation and request by client hence, JP TECHATRONICS or its employees should not be held responsible for any kind of malfunctioning of the system for any reasons.

Services like data backup, searching footage, port forwarding etc. to be charged as actuals.

Service calls post installation to be charged as actuals.