|  |  |  |  |
| --- | --- | --- | --- |
| **Active Components** | | | |
| **Sr. No** | **Model Number** | **Item Description** | **Qty** |
| 1 | DCS-F6123 | Dlink 12X 4 MP High Speed Dome Network Camera | 4 |
| 2 | DCS-F4712 | Dlink 2 MP Day & Night Fixed Outdoor Bullet Network Camera | 12 |
| 3 | DCS-F4724 | Dlink 4 MP Day & Night Varifocal Outdoor Bullet Network Camera | 4 |
| 4 | DNR F4864 | Dlink 64CH 8 SATA RAID Network Video Recorder (NVR) | 1 |
| 5 | DGS-1210-10P | Dlink 8-Ports 10/100/1000Mbps PoE + 2-Ports SFP 100/1000Mbps Smart Managed Switch, 65Watts | 1 |
| 6 | DGS-F1000-4P1T2S | Dlink 7 port Unmanged Switch with 4 x 10/100/1000 Base-T PoE+ Ports, 1 x 10/100/1000 Base-T Port & 2 x 100/1000 Base-X SFP port. -40°C~70°C (-40°F~158°F) Operating Temperature. | 4 |
| 7 | DEM-310GT | Dlink 1000Base-LX Single-Mode, 10KM SFP Transceiver | 2 |
| 8 | DEM-F310GTI | Dlink 1000Base-LX Single Mode SFP transceiver. 10 Km. -40° to 85° C operating temperature. | 8 |
| **Passive Components** | | | |
| **Sr. No** |  | **Item Description** | **Qty** |
| 1 | NWR-6U-5045-GR | Dlink Wall Mount Rack 6U x 550 W x 450 D, with Standard accessories | 1 |
| 2 | NPP-AL1BLK241 | Dlink Patch Panel UTP Keystone- 24 Port- Unloaded (Cat 5e,Cat 6 & Cat 6 A ) | 6 |
| 3 | NKJ-C6WHI1B21 | Dlink Jack Cat 6 Keystone UTP - White | 36 |
| 4 | NCB-C6UBLKR-305-O | Cabling with CAT 6 Dlink cable with casing, cabling, laying | 60 |
| 5 | NPG-5E1TRA031-100 | Dlink UTP Modular Plugs Pack of 100 | 1 |
| 6 | NCB-C6UGRYR1-1 | Dlink CAT6 UTP 24AWG PATCH CORD:1M,Plug 30U' Snagless | 36 |
| 7 | NCB-FS09O-AUHD-06 | Dlink O. F.Cable 06F Outdoor - Armoured Unitube SM - HDPE Sheath (qty in meters) with pulling/laying arially | 3000 |
| 8 | NLU-FSSLSCR-12 | Dlink LIU 12 Port Rack Mount - Loaded (SC) SM | 4 |
| 9 | NLU-FXXLXXR-06 | Dlink LIU 6 PORT Rack Mount - Loaded | 2 |
| 10 | NCB-FS09S-SC1 | Dlink PIGTAIL SC SM SIMPLEX LENGTH- 1m | 60 |
| 11 | NCB-FS09D-LCSC-1 | Dlink PATCH CORD LC-SC SM DUPLEX LENGTH- 1m | 10 |